Handling of bad commutation angle – now routine returns

Test correctness of voltage transformation, full motor control